Allegion

## Ask your question Entering your question as a complete sentence will provide more accurate results than keywords or phrases.

# “ maximum weight for auto operator ”

## RELATED FAQS

Question
Answer
What is maximum width, height and weight for IVES butt hinges?
Resolution: Butt hinges can be used on doors up to 4' wide and 200 pounds. There is no maximum door height, just need to add a hinge for every 30" or part there of over 7'.:
What is the maximum door weight recommended for LCN closers?
Resolution: The maximum recommended door weight for LCN closers is 225 lbs.:
How deep of a reveal will an 8200 Falcon Operator accommodate?
Resolution: The maximum reveal for an 8200 Falcon Operator is: 8230 (pull side) -- 1/8" 8240 (push side) -- 6" The Benchmark long rod and shoe (9140-79LR) can be use with the Falcon 8242 for reveal from ...:
What is maximum reveal for the 9140?
Resolution: Reveal should not exceed: 6" for the REGULAR ARM 9 3/4" for the LONG ARM:
What would cause a Senior Swing to open too far?
Resolution: The Senior Swing operator is designed to power open the door to 90°.
What is the minimum and maximum reveal for a 9500 Series Senior Swing operator?
Resolution: The 9542, 9553, 9563 surface mounted Senior Swing with a regular arm, mounted on the push side of the door, can handle a reveal from 1 1/8" up to 10". The 9542, 9553, 9563 surface mounted Senior S...:
What is the minimum and maximum PSI applied to a 4800 operator?
Resolution: The pneumatic operators are designed to function with an input air pressure to the 7901/7902 Series control box of 80 (min) 100 (max) PSI, and an output pressure of 60 to 80 PSI to the pneumatic (2...:
What is the maximum reveal for a regular arm 4642 operator?
Resolution: Max. reveal for a 4642: 4640 Regular arm -- 4.5" 4640 Long arm -- 8" 4640 x ST-3088 ( custom made - extra long rod) -- 8" to 11" No special mounting instructions required, just standard templ...: